Package: sara4r
Type: Package
Title: An R-GUI for Spatial Analysis of Surface Runoff using the
        NRCS-CN Method
Version: 0.1.0
Authors@R: c(person("Rafael", "Hernandez-Guzman", role=c("aut","cre"), email = "rhernandez.g@gmail.com", comment = c(ORCID ="0000-0002-2711-9015")), person("Arturo", "Ruiz-Luna", role=c("aut"), email = "arluna@ciad.mx", comment = c(ORCID ="0000-0001-6878-0929")))
Depends: R (>= 4.3.0), tcltk, tcltk2
Imports: terra
Maintainer: Rafael Hernandez-Guzman <rhernandez.g@gmail.com>
Description: A Graphical user interface to calculate the rainfall-runoff relation using the Natural Resources Conservation Service - Curve Number method (NRCS-CN method) but include modifications by Hawkins et al., (2002) about the Initial Abstraction. This GUI follows the programming logic of a previously published software (Hernandez-Guzman et al., 2011)<doi:10.1016/j.envsoft.2011.07.006>. It is a raster-based GIS tool that outputs runoff estimates from Land use/land cover and hydrologic soil group maps.
    This package has already been published in Journal of Hydroinformatics (Hernandez-Guzman et al., 2021)<doi:10.2166/hydro.2020.087> but it is under constant development at the Institute about Natural Resources Research (INIRENA) from the Universidad Michoacana de San Nicolas de Hidalgo and represents a collaborative effort between the Hydro-Geomatic Lab (INIRENA) with the Environmental Management Lab (CIAD, A.C.).
License: GPL (>= 3)
Encoding: UTF-8
URL: https://hydro-geomatic-lab.com/,
        https://hydro-geomatic-lab.com/sara4r.html
VignetteBuilder: knitr
Suggests: knitr, rmarkdown
RoxygenNote: 7.2.3
NeedsCompilation: no
Packaged: 2023-10-26 18:04:30 UTC; Veirus
Author: Rafael Hernandez-Guzman [aut, cre]
    (<https://orcid.org/0000-0002-2711-9015>),
  Arturo Ruiz-Luna [aut] (<https://orcid.org/0000-0001-6878-0929>)
Repository: CRAN
Date/Publication: 2023-10-26 20:10:02 UTC
Built: R 4.6.0; ; 2026-02-19 02:54:35 UTC; windows
